pictures 5 scale model line ship Santísima Trinidad

# 1/90 Scale model and diary

# line ship Santísima Trinidad

1 2 3 4 5

21. The "escobenes" of the anchor are walnut 8mm, a piece of 3,6x3,2 with the prow bend and the encounter with the bow stern.
The bowsprit and the prow figure head are only placed but not glued. The bow stern is walnut 8mm (wide of the San Juan Nepomuceno figure head AL).
The prow handrail is made of walnut 4x4, see plan cover nº2.

22. In this view you can observe the cover of the bulwark in walnut 5mm (sanded) and rounded in the encounters.

23. Placed the prow "beques" and the "apostles" of the bowsprit according to plane future of prow.

January 2003

24. General view with pedestal according to the plans.

25. MODEL IN REALIZATION..........

Anterior Siguiente