pictures 3 scale model line ship Santísima Trinidad

# 1/90 Scale model and diary

# line ship Santísima Trinidad

1 2 3 4 5

11. Prow simplified to place the armlets and the bottom board. It is not the final version

12. Prow simplified to place the armlets.

December 2002

13. The inferior part of the stern mirror has been placed in walnut 5mm and leaving that it has more than enough to both sides, this continuous piece the inferior bend of the stern (pictures 16 and 17) where the batteries are and where the helm enters. The bottom of the windows is made of dark blue bristol board and the divisions of the window are painted in black or brown, the pillars beside the windows are made of ramin of 3 or 4mm.
The stern balconys has stuck in two parts each one at the distances indicated in the section plane.
The comb (peineta) in walnut 5mm also in two parts, it is not still decorated (the center will be covered by a shield or figure) and the border are made of ramin 2x5mm.
The carpentry painted in bristol board has been glued and it has been plundered by lists of ramin2x2mm, and the pillars are in this covered with ramin 4x2

14. All the balconies placed, the pillars of the superior covers are of 3x3, the walnut " walls " are strips 0,6mm and the interior songs of the comb are made of ramin 0,6mm, except for the superior that is of 2mm.

15. The balustrades are of AL 10mm, according to the height you can cut the bases or to place them informs.
The hole in an oval way is appreciated where the helm is introduced.
The bristol board (in plastic paper) can receive the sealant varnish with the rest of the stern

Previous Next