pictures 2 scale model line ship Santísima Trinidad

# 1/90 Scale model and diary

# line ship Santísima Trinidad

1 2 3 4 5

November 2002

6. The 2nd deck already varnish, it is of plywood 3mm and later strips ramin 0.5mm, with bottom board for stairs to inferior deck, base mast and vent cooks (only that you can see).
the superior deck (forecastle and quarter-deck) it is made of strips, ramin 5mm then we place now the beam, walnut 4x4mm.

7. Placed the stringer (simple without figurehead) and stern post walnut 8mm and the keel 2 walnut, 2 ramin 5mm and 1 ramin 8mm, as well as the strips of the forecastle and quarter-deck: 1 walnut 5mm from here I place double strips 5mm in external and 6mm in internal (or what requests). 2 ramin 5mm. plus 1 ramin 5 mm in bow and 1 walnut 2mm - 3 ramin 5 mm in stern.

8. In the forecastle and quarter-deck accent the hole of 2 strips to port and starboard to be able to fix the cannons to the 2nd deck by eyebolts. We previously already had made the holes.

9. Poop with strips ramin 5mm, for under the lodgings are (already varnishings) in walnut.

In the following picture two cannons are presented (bigger of those than finally they will go in this deck) and a not finish stair, you can observe that it is necessary because in the section plan of the naval museum (nº 2) the stair is evened with the poop deck and its balustrade, the most correct position is the marked in the deck and boats plans (nº 3) because otherwise the stair would finish above the cannon

10. Simplified bow to place the armlets (this scale and smaller) as well as the hawse hole of the anchors.

Previous Next