1/12 scale FFVS J22 for Aircombat!

This one is built completely out of foam. The technique used is the same as 
for the P-40F that I have previously published on the net. For this reason
I will not publish another building-instruction, but you can instead use
the P40F instruction, and improvise wherever it is necessary.

A few piece of advise:

THIS ONE IS NOT FOR BEGINNERS!!!

Actually, THIS ONE IS NOT EVEN FOR MEDIOCRE R/C PILOTS!!!

You have to be a quite experienced 1/12 scale combat pilot to try
this one out. 

IS THIS CLEAR?


Ok, now when we've got that sorted out, another few pieces of advise:
- The wing should be enlarged so that the half stab span is 135millimeter
  (1 inch equals approximately 25 millimeter)
- Build light! This kite has a small wing, you need to keep the wingload down.
- The airfoil on the plan is an extreme one. You might want to change it to a more
  gentle one.
- Be careful NOT to forget the washout!
- With a hot engine, the J22 is a fast one! The kite is aerodynamically quite
  clean, and will be quick in all manouvres. Be prepared for this!


Finally I want to wish you the best of luck (you might need it!) !!!


/Martin Elmberg


The foam-blocks have the following measures (see the foam-block figure on how
the measures are laid out):

Partnbr	A	B	C	D	E
6	170	50	50	60	70
7	340	50	50	60	80
14	414	84/40	102/51	15	15
(All measures in millimeter)
For parts 6 and 7 measure A is an exact measure,
while the rest are min-measures.
For the two wingcores (14) measures A-C are exact measures,
while measures D-E are minmeasures. 
Please note that measures B-C differ on the different short-sides,
as the wing is tapered.
Centrelines are drawn onto the blocks using the above measures. 

List of numbered parts:
1. Fuselage template 1
2. Fuselage template 2
3. Fuselage template 3
4. Fuselage template 4
5. Fuselage template 5
6. Forward fuselage, foam
7. Rear fuselage, foam
8. Fin, 4mm balsa
9. Stab, 4mm balsa
10. Elevator, 4mm balsa
11. Engine mount, 3mm plywood
12. Rubberband dowels, 5mm dowel
13. Forward canopy, foam
14. Wingcore, foam
15. Leading edge, 10x15 balsa-spar
16. Wingtip, 15mm balsa
17. Trailing edge, 4x10 balsa
18. Aileron, 6x25 triangular stock
19. Wing sheeting, 1mm balsa
20. Inner template wing
21. Outer template wing

Materials-list:
Light foam, (white foam)
Higher density foam, (pink foam, etc)
4pcs 1x100x1000mm balsa
1pcs 4x100x1000mm balsa
1pcs 15x100x1000mm balsa
1pcs 3x100x1000mm plywood
1pcs 5mm dia rundstav
1pcs 10x15 balsa-spar
1pcs 4x10 balsa-spar
1pcs 6x25 triangular stock
