MOTOCOMPO

1 2 3 4

| Assembling of the body A part number 34 is cut and taken. Cut off the red line part of the photograph without forgetting it. Punching (6 place) is to have a blue line part.
| Assembling of the body Glue the front referring to the photograph.
| Assembling of the body Glue a back referring to the photograph.
| Assembling of the body It is installed in the body after a part number 35 is cut off and a curve is given as the photograph.
| Assembling of the body A part number 36.37 is cut off.
| Assembling of the body Install it in the body referring to the photograph.
| Assembling of the bumper 部品番号 38.39を切り取ります。 A bumper is to let me have roundness in accordance with the end part folding part. Though in fact it was an installation schedule in the last process, it
thinks that the one that it stuck here is easy to make.
| Assembling of the bumper It is the condition that a bumper is installed.
| Assembling of the body A body is installed in the body. Fit the one for the notched section in "Set" of the photograph to the installation position.
| Installation conditions
| Assembling around the gear box A part number 50.53 is cut off.
| Assembling around the gear box A part number 50 is assembled as the photograph and installed. A part number 53 is installed after it is bent as the photograph.
| Assembling around the gear box A part number 57 is cut off.
| Assembling around the gear box A part number 57 is assembled as the photograph and installed.
| Assembling of the license plate A part number 49 is cut off and assembled as the photograph.
| Assembling of the license plate Install it in the body referring to the photograph.
| Assembling of the headlights A part number 27 is cut off and assembled as the photograph.
| Assembling of the headlights Install it in the body referring to the photograph.
| Assembling of the seat Cut off a part number 40, and assemble it as the photograph.
| Assembling of the seat A part number 42 is cut off as the photograph. Punching is 1 place of the red line part.
| Assembling of the seat Part number 42 assembling conditions It is formed delicately with the part number 41, and put together. Assemble it carefully.
| Assembling of the seat 部品番号 41を写真のように切り取ります。 Punching is to go to 1 place (a red line part).
| Assembling of the seat Part number 41 assembling conditions Assemble it carefully with combining it with the part 42.
| Assembling of the seat It is combined as the photograph without gluing a part number 41 and 42. Confirm whether you move neatly.
| Assembling of the seat It sticks to the seat.
| Assembling of the seat It is installed in the body as the photograph. An installation position is to do referring to the parts list.

1 2 3 4