MOTOCOMPO

1 2 3 4

| Assembling around the engine A part number 54 is cut off. A punching point is to go referring to the photograph with 6 place in total.
| Assembling around the engine Bend a stand stopper as the photograph.
| Assembling around the engine It is cut off as the photograph after a part number 55 (stand) is laid.
| Assembling around the engine It tries to put a stand, and it is assembled. A stand isn't glued.
| Assembling around the engine It is installed in the body.
| Assembling around the rear A part number 51 is cut off. Do punching as the photograph in 1 place. After it is laid, a part number 52 is cut off as the photograph.
| Assembling around the rear A part number 52 is installed in 51.
| Assembling around the rear Install it in the body.
| The installation of the tire Install it referring to the photograph and the draft (parts list).
| Assembling of the ignition plug After a part number 56 is laid, it is cut off as the photograph.
| Assembling of the ignition plug They are the conditions that a part number 56 was installed in the body.
| Assembling of the exhaust muffler A part number 58 is cut off.
| Assembling of the exhaust muffler It is installed in the body with bending an exhaust pipe a little as the photograph.

1 2 3 4